


"Name" LLC

O R D E R


"__" ______ 2026 No. _____
On the Testing of Extension 
Ladders and Stepladders

Pursuant to Article 13 of the Law of Ukraine "On occupational health and safety" and clause 7.1. – clause 7.35. "Occupational Safety Rules for Work with Tools and Equipment" (NPAOP 0.00-1.71-13), and to prevent occupational injuries 


I ORDER: 


1. Appoint a commission for testing extension ladders and stepladders, consisting of: 

Chair of the Commission: Director Surname, Given Name, Patronymic

and commission members: Commercial director Surname, Given Name, Patronymic 
                                    Warehouse manager Surname, Given Name, Patronymic 


2. The Commission shall:
- to start work on testing extension ladders and stepladders in accordance with the procedure and intervals specified in clauses 7.1–7.35 of NPAOP 0.00-1.71-13; 
- draw up and approve the schedule for testing extension ladders and stepladders available at the enterprise;
- ensure proper registration of work results, as well as marking of ladders that have passed tests. 
3. Approve the Procedure for inspection and testing of portable ladders and stepladders (Attached).

4. I shall retain oversight of compliance with this Order.


          Director __________ Initials, Surname
  (signature)



I have read and understood the Order:
______________ ____________ Initials, Surname
           (date) (signature)                    

 "Name" LLC



TEST REPORT
Extension Ladder Test Report



Kyiv "_____"_______2026

 
The commission was appointed by the order dated 13.10.2026 No. 18-OHS, consisting of: 

Chair of the Commission: Director Surname, Given Name, Patronymic

and commission members: Commercial director Surname, Given Name, Patronymic 

                                    Warehouse manager Surname, Given Name, Patronymic

The Commission has drawn up this report on the testing of a metal/wooden extension ladder. 

During the test, the following was established: 

1. Description: metal/wooden extension ladder. 
2. Inventory number: ___________________________.
3. Date of commissioning: __________________.
4. Date of the last test __________________. 
5. Shop (site) where the ladder is used:_________________________.
6. Regulatory instrument, according to which the test is conducted: NPAOP 0.00-1.71-13 (clause 7.1 - clause 7.35). 
7. Procedure and type of test: 
static test, 2000 kg for 2 min.
8. Test results: no defects were found. 
9. Commission's conclusion: the ladder is fit/unfit for service. 


Chair of the Commission: Director ________________Surname, Given Name, Patronymic			

and commission members:  Commercial Director _____________ Surname, Given Name, Patronymic
 
                                   Warehouse manager ______________Surname, Given Name, Patronymic








"Name" LLC

Procedure for inspection and testing of portable ladders and stepladders
at "Name" LLC.


1. General provisions.

1.1. The procedure for inspection and testing of portable ladders and stepladders at "Name" LLC (hereinafter referred to as the Procedure) sets out the procedure for inspecting, checking and testing of portable ladders and stepladders at "Name" LLC (hereinafter referred to as the enterprise). 
1.2. The requirements of the Procedure apply to all structural divisions of the enterprise.
1.3. Maintenance, operation and testing of portable ladders and stepladders are carried out in accordance with the requirements of their technical (operational) documentation - technical data sheet and/or instructions from the manufacturer of ladders and stepladders and in accordance with the provisions of regulatory and legal documents.
Storage and operation at the enterprise of portable ladders and stepladders (hereinafter referred to as ladders/stepladders) that are not recorded in the on- or off-balance-sheet asset registers (not inventoried) and have not been tested are prohibited. 
1.3. The Commission established by order shall organize and conduct the testing of portable ladders and stepladders at the enterprise. 
1.4. The responsibility for accounting, operation and control of the technical condition, inspection and testing of ladders/stepladders rests with the heads of structural units.
1.5. Depending on the specifics of the activity of the structural unit, the presence of subordinate units, the number of registered ladders and stepladders, the conditions of their operation, the head of the structural unit shall, by directive, appoint a person responsible for inventory control and the safe condition of portable ladders and stepladders, from among competent (engineering and technical) employees. 

2. Inspection of Portable Ladders and Stepladders.

2.1. In the process of operation, ladders/stepladders are subject to inspections for compliance with safety requirements. 2.2. A visual inspection of the ladder/stepladder is performed personally by the employee immediately before its use (without recording the results). 
In case of detection of deficiencies, damages and malfunctions, the employee is obliged to notify the person responsible for inventory control and the safe condition of the ladder/stepladder or the head of the unit, and shall not use the defective ladder/stepladder. 
2.3. The head of the structural unit is obliged to provide maintenance, timely repair, and replacement of elements and components that are damaged, defective, missing, or have lost their properties. In the case of detection of defects in the construction of a ladder/stepladder that cannot technically be repaired, such a ladder/stepladder is written off from the balance sheet of the enterprise, in accordance with the procedure established by law. 
2.4. If defects and malfunctions are found in the ladder/stepladder, their use is prohibited and measures are taken to warn other workers about this. 

3. Testing portable ladders and stepladders.

3.1. Ladders/stepladders shall be tested in accordance with this Procedure unless different specific testing requirements are prescribed in the manufacturer's technical (operating) documentation—technical data sheet and/or instructions. 
3.2. All ladders/stepladders are subject to mandatory static load testing (hereinafter referred to as testing). 
3.3. The initial tests of the ladder/stepladder are carried out during its commissioning (entry into the asset register). 
3.4. Scheduled tests shall be conducted at the following intervals: metal ladders and stepladders—once every 12 months; wooden ladders and stepladders—once every 6 months; suspended rope ladders—once every 6 months. Planned tests of ladders/stepladders are carried out according to approved schedules drawn up by the person responsible for organizing and conducting tests of ladders and stepladders at the enterprise. 
3.5. Unscheduled tests of ladders/stepladders are carried out after their repair, by order of the person responsible for organizing and conducting tests of portable ladders and stepladders. 
3.6. Before each test, the ladder/stepladder shall first undergo a mandatory technical inspection. 
3.7. If the inspection results are positive, the ladder/stepladder may be tested. 
3.8. If the results of the ladder/stepladder inspection are unsatisfactory, testing is prohibited until all violations and deficiencies have been fully corrected. 
3.9. If damage, cracks, deformation or other defects are found in the ladder/stepladder after static testing, it must be repaired, after which the inspection and testing procedure is repeated. 
3.10. If, during the inspection or after the tests, defects or damage that cannot technically be repaired are found in the ladder/stepladder, then such a ladder/stepladder is written off from the company's balance sheet. 
3.11. According to the results of the tests (positive, unsatisfactory), the Testing Commission shall prepare a Test Report for the wooden (metal) portable ladder/stepladder. Test reports shall be retained in the structural subdivisions where ladders/stepladders are registered, until they are replaced with new ones. 

4. The procedure for conducting tests of ladders and stepladders. 

4.1. Testing of portable ladders and stepladders is carried out by the Testing Commission.

4.2. The ladder/stepladder is tested by hanging a static load from its rungs and stringers. 
During testing, all employees comply with safety requirements.

4.3. Testing of the stepladder (wooden and metal).
The tests are carried out in accordance with the requirements of the operational documentation - the technical data sheet (instructions) for the stepladder from the manufacturer. 
If the test requirements are not specified in the technical data sheet (instructions), the tests are carried out as follows: 
1) the stepladder is installed in the working position on a level horizontal surface; 
2) a load of 1.2 kN (120 kgf) is suspended from the midpoint of an unreinforced rung in the middle part; test duration - 2 min. If during the inspection there are doubts about the safe condition of certain rungs, then they shall be tested individually. 
3) If both sections of the stepladder have rungs, each section shall be tested separately. If the second section serves only as a support, only its stringers shall be tested. 
4) the stringers of both sections shall be tested in turn: a load of 1 kN (100 kgf) is suspended from each stringer at the midpoint of the section; test duration - 2 min. 

4.4. Testing of extension and sectional extension ladders.
The tests are carried out in accordance with the requirements of the operational documentation - the technical data sheet for the ladder from the manufacturer. 
If the requirements for the tests are not specified in the technical data sheet, the tests are carried out in the following way: 
1) the ladder is set up on a firm, level base and leaned against a wall or structure at an angle of 60° to the horizontal plane; 
2) a load of 1.2 kN (120 kgf) is suspended from the middle part of the unreinforced rung in the middle section of the ladder; test duration - 2 min. If during the inspection there are doubts about the safe condition of certain rungs, then they shall be tested individually. 3) stringer test: a load of 1 kN (100 kgf) is suspended from both stringers in the midpoint of the section; test duration - 2 min. 

4.5. Sliding ladder test.
Tests are carried out in accordance with the requirements of operational documentation - technical data sheet (instructions) for the ladder from the manufacturer. 
If the test requirements are not specified in the technical data sheet (instructions), the tests are carried out as follows: 
1) the sliding ladder is installed on a solid base and attached to the wall or structure at an angle of 60° to the horizontal plane; the three-section ladder must be fully extended. 
2) a load of 2 kN (200 kgf) is suspended from the midpoint of an unreinforced rung of the lower section of the ladder; test duration - 2 min.; If during the inspection there are doubts about the safe condition of certain rungs, then they shall be tested individually. 
3) stringers are tested in two ways: 
- first, a load of 1 kN (100 kgf) is applied to each of them in the middle; all sections are tested in turn; test duration - 2 min.; 
- after removing the load, a load of 2 kN (200 kgf) is suspended from both stringers in the midpoint of the middle section (it can be suspended from the middle rung); test duration - 2 min. After testing, the sections of the sliding ladder shall extend and retract freely. 
4) during tests of chains, hooks and locking devices, the sliding ladder is hung vertically by the hooks, and a load of 2 kN (200 kgf) is hung from the bottom rung of the ladder; test duration - 2 min. After removing the load, there should be no cracks in the places of welding of chain links, as well as deformation of welded links and locking devices. 

4.6. Collapsible ladder testing.
Installation, operation and testing of the collapsible ladder are carried out in accordance with the requirements of the operational documentation - the technical data sheet (instructions) of the ladder from the manufacturer. 
If the test requirements are not specified in the technical data sheet (instructions), the tests are carried out as follows: 
1) test sections: a load of 2 kN (200 kgf) is suspended to the rungs at two points in the middle and at the attachment point to the support; test duration - 2 min.; 
2) after assembly and installation of the ladder, a load of 2 kN (200 kgf) is suspended from the upper rung of the lower (seventh) section; test duration - 5 min. After removing the load, there should be no deformation, cracks or other damage that reduces the mechanical strength of such ladders. 

4.7. Testing of rope and metal suspension ladders. 
Installation, operation and testing of rope and metal suspension ladders are carried out in accordance with the requirements of operational documentation - the technical data sheet (instructions) of the ladder from the manufacturer. 
If the test requirements are not specified in the technical data sheet (instructions), the tests are carried out as follows: 
1) the ladder is hung vertically and fixed to the structure with two grips;
2) a load of 1.2 kN (120 kgf) is suspended to the middle of the lower rung; test duration - 2 min.; 
3) If a metal ladder has a work platform, it is tested: a load of 1.2 kN (120 kgf) is suspended from this platform; test duration - 2 min. In the absence of conditions for carrying out tests of suspension ladders in the working (vertical) position, they can be tested under tension in a horizontal position, in this case controlling the load with a dynamometer. 

4.8. Testing of other types of portable ladders for special purposes, mobile ladders, telescopic ladders, and transformer ladders is carried out in accordance with the requirements of the operating documentation - the technical data sheet of the ladder from the manufacturer. In the absence of operational documentation for such types of ladders, their operation at the enterprise is prohibited.  



Developed by: The person responsible for the work on 
                                 height (work from ladders and stepladders) ______________ Initials, Surname

Agreed:    
                                 occupational safety engineer ______________ Initials, Surname
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